tmp Thu Oct 02 10:53:33 2003 1

mysql> select caid, title, duration from ioc_tasks where campn0=’Q’ order by camp_ord;
+------+-----------------------------------------------------+----------+
| caid | title                                               | duration |
+------+-----------------------------------------------------+----------+
|  905 | Start-up Activities, Si & Ge                        |       40 |
|  912 | IOC Darks, 160 um                                   |       17 |
|  911 | IOC Darks - 70 um                                   |       33 |
|  910 | IOC Darks, 24 um                                    |       17 |
|  307 | 160 um IC - detailed, Scan AOR                      |       66 |
|  306 | 70 um IC - detailed, Scan AOR                       |       66 |
|  305 | 24 um Flat - detailed, Scan AOR                     |       66 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  924 | 160 um Flux Standards                               |       11 |
|  920 | 24 um Flux Standards                                |        7 |
|  922 | 70 um Flux Standards                                |        7 |
|  192 | Dark Verification, 160 um                           |       21 |
|  150 | Observing Mode Relative Throughputs                 |      135 |
|  190 | Dark Verification, 24 um                            |       28 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  328 | Scan AOT Validation - slow speed                    |      442 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  317 | Off-Axis Glints                                     |      499 |
|  962 | 70 um NF Frame Table Update Sanity Check            |        5 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  600 | Flux-Nonlinearity Calibration, 70 and 160 um Arrays |      146 |
|  300 | SED Skeleton AOT Validation                         |       58 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  919 | 160 um IC - routine, Phot AOR                       |       24 |
|  924 | 160 um Flux Standards                               |       11 |
|  918 | 70 um IC - routine, Phot AOR                        |       24 |
|  313 | 70 um NF Illumination Correction                    |       23 |
|  299 | SED Slit Illumination Function                      |       19 |
|  133 | 70 um WF Focal Plane Survey (Fine)                  |      107 |
|  922 | 70 um Flux Standards                                |        7 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  930 | Ge Anneal and Recovery                              |       15 |
|  235 | 160 um array geometry                               |      374 |
|  160 | 70 and 160 um Thermal Anneal Behavior               |      388 |
|  131 | 24 um Focal Plane Survey (Fine) #1                  |      167 |
|  992 | Shut-down Activities, Ge (& Si)                     |       23 |
+------+-----------------------------------------------------+----------+